**Product Data Sheet.**

**Ratchet Cargo Lashing Tie Downs. Ratchet Straps. Cargo Straps**

1. Assembly manufactured in accordance with EN 12195-2:2001
2. Webbing manufactured from Polyethylene PES with stretch factor of less than 7%.
3. Blue vinyl label sewn in to both loose parts of webbing
4. Webbing manufactured to withstand 50% increase in stated strength

**Caring for Cargo Straps.**

1. Inspect webbing before and after use, for scuffs, nicks, tears or unknown stains.
2. Keep Cargo Straps rolled up and in a safe place when not in use
3. Make sure that the blue labels are intact and legible
4. Regularly check the ratchet and hardware for distortion, rusting or fractures
5. Wash Cargo Straps in clean water with mild detergent and allow to drip dry.
6. Never use bars or levers to increase the tension on a ratchet
7. Always use edge protectors or wear sleeves over rough or sharp edges
8. Check the blue label for the lashing capacity before using, and ensure the correct number of Cargo Straps are used
9. Do not use Cargo Straps that are damaged or worn out.
10. Keep Cargo Straps well away from harmful substances.

**NEVER USE CARGOSTRAPS IN THE FOLLOWING CONDITION!**

1. Knotted
2. Nicked or cut
3. Frayed, abraded or scuffed
4. Stained, where the reason for the stain is not known and could be detrimental to the webbing fibres.

**IF IN DOUBT – THROW THEM OUT!**

This Product and Safety Data Sheet has been compiled for free issue with Cargo Straps.